/*
*****************************************************************************
**

**  File        : LinkerScript.ld
**
**  Abstract    : Linker script for STM32L476RGTx Device with
**                0KByte FLASH, 0KByte RAM
**
**                Set heap size, stack size and stack location according
**                to application requirements.
**
**                Set memory bank area and size if external memory is used.
**
**  Target      : STMicroelectronics STM32
**
**
**  Distribution: The file is distributed as is, without any warranty
**                of any kind.
**
**  (c)Copyright Ac6.
**  You may use this file as-is or modify it according to the needs of your
**  project. Distribution of this file (unmodified or modified) is not
**  permitted. Ac6 permit registered System Workbench for MCU users the
**  rights to distribute the assembled, compiled & linked contents of this
**  file as part of an application binary file, provided that it is built
**  using the System Workbench for MCU toolchain.
**
*****************************************************************************
*/

/* Slots Regions must be aligned on 2048 bytes (0x800) */

/* swap region : 0x2000 (8kbytes) */
__ICFEDIT_region_SWAP_start__   = 0x080F2800;
__ICFEDIT_region_SWAP_end__     = 0x080F47FF;

/* slot 0 region : 0x70000 (448kbytes) */
__ICFEDIT_region_SLOT_0_start__ = 0x08080800;
__ICFEDIT_region_SLOT_0_end__   = 0x080F07FF;

/* slot 1 region : 0x70000 (448kbytes) */
__ICFEDIT_region_SLOT_1_start__ = 0x08010000; /* step 2 */
__ICFEDIT_region_SLOT_1_end__   = 0x0807FFFF;

