#MicroXplorer Configuration settings - do not modify
CAD.formats=
CAD.pinconfig=
CAD.provider=
CORTEX_M33_NS.userName=CORTEX_M33
DCACHE1.DCACHE_Read_Burst_Type=DCACHE_READ_BURST_INCR
DCACHE1.IPParameters=DCACHE_Read_Burst_Type
DCACHE2.DCACHE_Read_Burst_Type=DCACHE_READ_BURST_INCR
DCACHE2.IPParameters=DCACHE_Read_Burst_Type
DMA2D.ColorMode=DMA2D_OUTPUT_RGB888
DMA2D.IPParameters=Mode,ColorMode
DMA2D.Mode=DMA2D_R2M
File.Version=6
GPDMA1.DATAALIGNEMENT_GPDMACH0=DMA_DATA_PACK
GPDMA1.DATAHANDLING_GPDMACH0=ENABLE
GPDMA1.DATAHANDLING_GPDMACH1=NONE
GPDMA1.DESTBURSTLENGTH_GPDMACH0=8
GPDMA1.DESTBURSTLENGTH_GPDMACH1=8
GPDMA1.DESTDATAWIDTH_GPDMACH0=DMA_DEST_DATAWIDTH_WORD
GPDMA1.DESTDATAWIDTH_GPDMACH1=DMA_DEST_DATAWIDTH_WORD
GPDMA1.DESTINC_GPDMACH1=DMA_DINC_INCREMENTED
GPDMA1.DIRECTION_GPDMACH0=DMA_MEMORY_TO_PERIPH
GPDMA1.IPHANDLE_GPDMACH0-SIMPLEREQUEST_GPDMACH0=__NULL
GPDMA1.IPHANDLE_GPDMACH1-SIMPLEREQUEST_GPDMACH1=__NULL
GPDMA1.IPParameters=IPHANDLE_GPDMACH0-SIMPLEREQUEST_GPDMACH0,REQUEST_GPDMACH0,DIRECTION_GPDMACH0,SRCINC_GPDMACH0,SRCBURSTLENGTH_GPDMACH0,TRANSFERALLOCATEDPORTSRC_GPDMACH0,DESTDATAWIDTH_GPDMACH0,DESTBURSTLENGTH_GPDMACH0,IPHANDLE_GPDMACH1-SIMPLEREQUEST_GPDMACH1,REQUEST_GPDMACH1,SRCDATAWIDTH_GPDMACH1,SRCBURSTLENGTH_GPDMACH1,DESTINC_GPDMACH1,DESTDATAWIDTH_GPDMACH1,DESTBURSTLENGTH_GPDMACH1,TRANSFERALLOCATEDPORTDEST_GPDMACH1,DATAHANDLING_GPDMACH1,DATAHANDLING_GPDMACH0,DATAALIGNEMENT_GPDMACH0,PRIORITY_GPDMACH1,PRIORITY_GPDMACH0
GPDMA1.PRIORITY_GPDMACH0=DMA_HIGH_PRIORITY
GPDMA1.PRIORITY_GPDMACH1=DMA_HIGH_PRIORITY
GPDMA1.REQUEST_GPDMACH0=GPDMA1_REQUEST_JPEG_RX
GPDMA1.REQUEST_GPDMACH1=GPDMA1_REQUEST_JPEG_TX
GPDMA1.SRCBURSTLENGTH_GPDMACH0=8
GPDMA1.SRCBURSTLENGTH_GPDMACH1=8
GPDMA1.SRCDATAWIDTH_GPDMACH1=DMA_SRC_DATAWIDTH_WORD
GPDMA1.SRCINC_GPDMACH0=DMA_SINC_INCREMENTED
GPDMA1.TRANSFERALLOCATEDPORTDEST_GPDMACH1=DMA_DEST_ALLOCATED_PORT1
GPDMA1.TRANSFERALLOCATEDPORTSRC_GPDMACH0=DMA_SRC_ALLOCATED_PORT1
GPIO.groupedBy=Group By Peripherals
HSPI1.ChipSelectHighTimeCycle=2
HSPI1.ClockPrescaler=0
HSPI1.DelayBlockBypass=HAL_XSPI_DELAY_BLOCK_BYPASS
HSPI1.DeviceType=SPI_DEVICE_FLASH
HSPI1.FifoThresholdByte=4
HSPI1.IPParameters=DeviceType,MemoryType,FifoThresholdByte,MemorySize,ChipSelectHighTimeCycle,DelayBlockBypass,ClockPrescaler
HSPI1.MemorySize=HAL_XSPI_SIZE_1GB
HSPI1.MemoryType=HAL_XSPI_MEMTYPE_MACRONIX
I2C2.I2C_Speed_Mode=I2C_Fast
I2C2.IPParameters=Timing,I2C_Speed_Mode
I2C2.Timing=0x00F07BFF
JPEG.IPParameters=USE_JPEG_ENCODER,JPEG_RGB_FORMAT
JPEG.JPEG_RGB_FORMAT=JPEG_RGB565
JPEG.USE_JPEG_ENCODER=0
KeepUserPlacement=false
LTDC.ActiveW=800
LTDC.Alpha_L0=255
LTDC.HBP=8
LTDC.HFP=8
LTDC.HSync=5
LTDC.IPParameters=ActiveW,HSync,HBP,HFP,VSync,VBP,VFP,Layers,WindowX1_L0,WindowY1_L0,PixelFormat_L0,Alpha_L0,ImageWidth_L0,ImageHeight_L0
LTDC.ImageHeight_L0=480
LTDC.ImageWidth_L0=800
LTDC.Layers=0
LTDC.PixelFormat_L0=LTDC_PIXEL_FORMAT_RGB565
LTDC.VBP=8
LTDC.VFP=14
LTDC.VSync=5
LTDC.WindowX1_L0=800
LTDC.WindowY1_L0=480
MMTAppRegionsCount=0
MMTConfigApplied=false
Mcu.CPN=STM32U5G9ZJT6Q
Mcu.ContextProject=TrustZoneDisabled
Mcu.Family=STM32U5
Mcu.IP0=CORTEX_M33_NS
Mcu.IP1=CRC
Mcu.IP10=JPEG
Mcu.IP11=LPBAM
Mcu.IP12=LPBAMQUEUE
Mcu.IP13=LTDC
Mcu.IP14=MEMORYMAP
Mcu.IP15=NVIC
Mcu.IP16=PWR
Mcu.IP17=RCC
Mcu.IP18=SYS
Mcu.IP2=DCACHE1
Mcu.IP3=DCACHE2
Mcu.IP4=DMA2D
Mcu.IP5=GPDMA1
Mcu.IP6=GPU2D
Mcu.IP7=HSPI1
Mcu.IP8=I2C2
Mcu.IP9=ICACHE
Mcu.IPNb=19
Mcu.Name=STM32U5G9ZJTxQ
Mcu.Package=LQFP144
Mcu.Pin0=PE4
Mcu.Pin1=PE5
Mcu.Pin10=PE7
Mcu.Pin11=PE8
Mcu.Pin12=PE9
Mcu.Pin13=PE10
Mcu.Pin14=PE11
Mcu.Pin15=PE12
Mcu.Pin16=PE13
Mcu.Pin17=PE14
Mcu.Pin18=PE15
Mcu.Pin19=PD8
Mcu.Pin2=PE6
Mcu.Pin20=PD9
Mcu.Pin21=PD10
Mcu.Pin22=PD11
Mcu.Pin23=PD12
Mcu.Pin24=PD13
Mcu.Pin25=PD14
Mcu.Pin26=PD15
Mcu.Pin27=PH9
Mcu.Pin28=PH10
Mcu.Pin29=PH11
Mcu.Pin3=PC13
Mcu.Pin30=PH12
Mcu.Pin31=PH13
Mcu.Pin32=PH14
Mcu.Pin33=PH15
Mcu.Pin34=PI0
Mcu.Pin35=PI1
Mcu.Pin36=PI2
Mcu.Pin37=PI3
Mcu.Pin38=PC6
Mcu.Pin39=PC7
Mcu.Pin4=PF0
Mcu.Pin40=PC8
Mcu.Pin41=PC9
Mcu.Pin42=PC10
Mcu.Pin43=PC11
Mcu.Pin44=PC12
Mcu.Pin45=PD0
Mcu.Pin46=PD1
Mcu.Pin47=PD2
Mcu.Pin48=PD3
Mcu.Pin49=PD4
Mcu.Pin5=PF1
Mcu.Pin50=PD6
Mcu.Pin51=PB9
Mcu.Pin52=PE0
Mcu.Pin53=VP_CRC_VS_CRC
Mcu.Pin54=VP_DCACHE1_VS_DCACHE
Mcu.Pin55=VP_DCACHE2_VS_DCACHE
Mcu.Pin56=VP_DMA2D_VS_DMA2D
Mcu.Pin57=VP_GPDMA1_VS_GPDMACH0
Mcu.Pin58=VP_GPDMA1_VS_GPDMACH1
Mcu.Pin59=VP_GPU2D_VS_GPU2D
Mcu.Pin6=PH0-OSC_IN (PH0)
Mcu.Pin60=VP_ICACHE_VS_ICACHE
Mcu.Pin61=VP_JPEG_VS_JPEG
Mcu.Pin62=VP_LPBAMQUEUE_VS_QUEUE
Mcu.Pin63=VP_PWR_VS_DBSignals
Mcu.Pin64=VP_PWR_VS_SECSignals
Mcu.Pin65=VP_PWR_VS_LPOM
Mcu.Pin66=VP_SYS_VS_tim6
Mcu.Pin67=VP_LPBAM_VS_SIG1
Mcu.Pin68=VP_LPBAM_VS_SIG4
Mcu.Pin69=VP_MEMORYMAP_VS_MEMORYMAP
Mcu.Pin7=PH1-OSC_OUT (PH1)
Mcu.Pin70=VP_STMicroelectronics.X-CUBE-FREERTOS_VS_CMSISJjRTOS2_10.4.6_1.0.1
Mcu.Pin71=VP_STMicroelectronics.X-CUBE-TOUCHGFX_VS_GraphicsJjApplication_4.24.1
Mcu.Pin8=PC0
Mcu.Pin9=PB2
Mcu.PinsNb=72
Mcu.ThirdParty0=STMicroelectronics.X-CUBE-FREERTOS.1.0.1
Mcu.ThirdParty1=STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1
Mcu.ThirdPartyNb=2
Mcu.UserConstants=
Mcu.UserName=STM32U5G9ZJTxQ
MxCube.Version=6.12.0
MxDb.Version=DB.6.0.120
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.DMA2D_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.EXTI5_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.ForceEnableDMAVector=true
NVIC.GPDMA1_Channel0_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC.GPDMA1_Channel1_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC.GPU2D_ER_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.GPU2D_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.HSPI1_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.JPEG_IRQn=true\:7\:0\:true\:false\:true\:true\:true\:true\:true
NVIC.LTDC_ER_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.LTDC_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=true
NVIC.SavedSvcallIrqHandlerGenerated=true
NVIC.SavedSystickIrqHandlerGenerated=true
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:true\:false
NVIC.TIM6_IRQn=true\:0\:0\:true\:false\:true\:false\:false\:true\:true
NVIC.TimeBase=TIM6_IRQn
NVIC.TimeBaseIP=TIM6
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
PB2.Mode=RGB888
PB2.Signal=LTDC_B1
PB9.Mode=RGB888
PB9.Signal=LTDC_B0
PC0.GPIOParameters=GPIO_Speed,GPIO_Label
PC0.GPIO_Label=VSYNC_FREQ
PC0.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PC0.Locked=true
PC0.Signal=GPIO_Output
PC10.GPIOParameters=GPIO_Speed,GPIO_Label
PC10.GPIO_Label=RENDER_TIME
PC10.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PC10.Locked=true
PC10.Signal=GPIO_Output
PC11.GPIOParameters=GPIO_Speed,GPIO_Label
PC11.GPIO_Label=FRAME_RATE
PC11.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PC11.Locked=true
PC11.Signal=GPIO_Output
PC12.GPIOParameters=GPIO_Speed,GPIO_Label
PC12.GPIO_Label=MCU_ACTIVE
PC12.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PC12.Locked=true
PC12.Signal=GPIO_Output
PC13.GPIOParameters=GPIO_PuPd,GPIO_Label
PC13.GPIO_Label=USER_BUTTON
PC13.GPIO_PuPd=GPIO_PULLDOWN
PC13.Locked=true
PC13.Signal=GPIO_Input
PC6.Locked=true
PC6.Mode=RGB888
PC6.Signal=LTDC_R0
PC7.Locked=true
PC7.Mode=RGB888
PC7.Signal=LTDC_R1
PC8.Locked=true
PC8.Mode=RGB888
PC8.Signal=LTDC_G0
PC9.Locked=true
PC9.Mode=RGB888
PC9.Signal=LTDC_G1
PD0.Mode=RGB888
PD0.Signal=LTDC_B4
PD1.Mode=RGB888
PD1.Signal=LTDC_B5
PD10.Mode=RGB888
PD10.Signal=LTDC_R5
PD11.Mode=RGB888
PD11.Signal=LTDC_R6
PD12.Mode=RGB888
PD12.Signal=LTDC_R7
PD13.GPIOParameters=GPIO_Speed,GPIO_Mode
PD13.GPIO_Mode=GPIO_MODE_AF_PP
PD13.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PD13.Locked=true
PD13.Mode=RGB888
PD13.Signal=LTDC_VSYNC
PD14.Mode=RGB888
PD14.Signal=LTDC_B2
PD15.Mode=RGB888
PD15.Signal=LTDC_B3
PD2.GPIOParameters=GPIO_Speed,PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PD2.GPIO_Label=USER_LD2_RED
PD2.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PD2.GPIO_PuPd=GPIO_NOPULL
PD2.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PD2.Locked=true
PD2.PinState=GPIO_PIN_SET
PD2.Signal=GPIO_Output
PD3.GPIOParameters=GPIO_Speed
PD3.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PD3.Locked=true
PD3.Mode=RGB888
PD3.Signal=LTDC_CLK
PD4.GPIOParameters=GPIO_Speed,PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PD4.GPIO_Label=USER_LD3_GREEN
PD4.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PD4.GPIO_PuPd=GPIO_NOPULL
PD4.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PD4.Locked=true
PD4.PinState=GPIO_PIN_SET
PD4.Signal=GPIO_Output
PD6.Mode=RGB888
PD6.Signal=LTDC_DE
PD8.Mode=RGB888
PD8.Signal=LTDC_R3
PD9.Mode=RGB888
PD9.Signal=LTDC_R4
PE0.GPIOParameters=GPIO_Speed
PE0.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PE0.Locked=true
PE0.Mode=RGB888
PE0.Signal=LTDC_HSYNC
PE10.Mode=RGB888
PE10.Signal=LTDC_G3
PE11.Mode=RGB888
PE11.Signal=LTDC_G4
PE12.Mode=RGB888
PE12.Signal=LTDC_G5
PE13.Mode=RGB888
PE13.Signal=LTDC_G6
PE14.Mode=RGB888
PE14.Signal=LTDC_G7
PE15.Mode=RGB888
PE15.Signal=LTDC_R2
PE4.GPIOParameters=PinState,GPIO_Label
PE4.GPIO_Label=LCD_DISP_EN
PE4.Locked=true
PE4.PinState=GPIO_PIN_SET
PE4.Signal=GPIO_Output
PE5.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultEXTI
PE5.GPIO_Label=TP_IRQ
PE5.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_FALLING
PE5.GPIO_PuPd=GPIO_PULLUP
PE5.Locked=true
PE5.Signal=GPXTI5
PE6.GPIOParameters=PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PE6.GPIO_Label=LCD_BL_CTRL
PE6.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PE6.GPIO_PuPd=GPIO_NOPULL
PE6.Locked=true
PE6.PinState=GPIO_PIN_SET
PE6.Signal=GPIO_Output
PE7.Mode=RGB888
PE7.Signal=LTDC_B6
PE8.Mode=RGB888
PE8.Signal=LTDC_B7
PE9.Mode=RGB888
PE9.Signal=LTDC_G2
PF0.Mode=I2C
PF0.Signal=I2C2_SDA
PF1.Mode=I2C
PF1.Signal=I2C2_SCL
PH0-OSC_IN\ (PH0).Mode=HSE-External-Oscillator
PH0-OSC_IN\ (PH0).Signal=RCC_OSC_IN
PH1-OSC_OUT\ (PH1).Mode=HSE-External-Oscillator
PH1-OSC_OUT\ (PH1).Signal=RCC_OSC_OUT
PH10.Mode=octo_mode
PH10.Signal=HSPI1_IO0
PH11.Mode=octo_mode
PH11.Signal=HSPI1_IO1
PH12.Mode=octo_mode
PH12.Signal=HSPI1_IO2
PH13.Mode=octo_mode
PH13.Signal=HSPI1_IO3
PH14.Mode=octo_mode
PH14.Signal=HSPI1_IO4
PH15.Mode=octo_mode
PH15.Signal=HSPI1_IO5
PH9.Mode=octo_mode
PH9.Signal=HSPI1_NCS
PI0.Mode=octo_mode
PI0.Signal=HSPI1_IO6
PI1.Mode=octo_mode
PI1.Signal=HSPI1_IO7
PI2.Mode=octo_mode
PI2.Signal=HSPI1_DQS0
PI3.Mode=octo_mode
PI3.Signal=HSPI1_CLK
PWR.IPParameters=PowerMode
PWR.PowerMode=PWR_SMPS_SUPPLY
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32U5G9ZJTxQ
ProjectManager.FirmwarePackage=STM32Cube FW_U5 V1.6.0
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x1000
ProjectManager.KeepUserCode=true
ProjectManager.LPBAM.generateCode=
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=STM32U5G9J-DK2.ioc
ProjectManager.ProjectName=STM32U5G9J-DK2
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x1000
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=false
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false,2-MX_GPIO_Init-GPIO-false-HAL-true,3-MX_GPDMA1_Init-GPDMA1-false-HAL-true,4-MX_ICACHE_Init-ICACHE-false-HAL-true,5-MX_DCACHE1_Init-DCACHE1-false-HAL-true,6-MX_DCACHE2_Init-DCACHE2-false-HAL-true,7-MX_CRC_Init-CRC-false-HAL-true,8-MX_LTDC_Init-LTDC-false-HAL-true,9-MX_DMA2D_Init-DMA2D-false-HAL-true,10-MX_GPU2D_Init-GPU2D-false-HAL-true,11-MX_HSPI1_Init-HSPI1-false-HAL-true,12-MX_I2C2_Init-I2C2-false-HAL-true,13-MX_JPEG_Init-JPEG-false-HAL-true,16-MX_TouchGFX_Init-STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1-false-HAL-false,17-MX_TouchGFX_Process-STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1-false-HAL-false,0-MX_CORTEX_M33_NS_Init-CORTEX_M33_NS-false-HAL-true,0-MX_PWR_Init-PWR-false-HAL-true
RCC.ADCFreq_Value=16000000
RCC.ADF1Freq_Value=160000000
RCC.AHBFreq_Value=160000000
RCC.APB1Freq_Value=160000000
RCC.APB1TimFreq_Value=160000000
RCC.APB2Freq_Value=160000000
RCC.APB2TimFreq_Value=160000000
RCC.APB3Freq_Value=160000000
RCC.CK48Freq_Value=48000000
RCC.CRSFreq_Value=48000000
RCC.CortexFreq_Value=160000000
RCC.DACFreq_Value=32000
RCC.DSICLockSelection=RCC_DSICLKSOURCE_PLL3
RCC.DSIFreq_Value=62500000
RCC.DSITXEscFreq_Value=15625000
RCC.EPOD_VALUE=16000000
RCC.FCLKCortexFreq_Value=160000000
RCC.FDCANFreq_Value=160000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=160000000
RCC.HSE_VALUE=16000000
RCC.HSI48_VALUE=48000000
RCC.HSI_VALUE=16000000
RCC.HSPI1Freq_Value=132000000
RCC.HSPICLockSelection=RCC_HSPICLKSOURCE_PLL2
RCC.I2C1Freq_Value=160000000
RCC.I2C2Freq_Value=160000000
RCC.I2C3Freq_Value=160000000
RCC.I2C4Freq_Value=160000000
RCC.I2C5Freq_Value=160000000
RCC.I2C6Freq_Value=160000000
RCC.IPParameters=ADCFreq_Value,ADF1Freq_Value,AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,APB3Freq_Value,CK48Freq_Value,CRSFreq_Value,CortexFreq_Value,DACFreq_Value,DSICLockSelection,DSIFreq_Value,DSITXEscFreq_Value,EPOD_VALUE,FCLKCortexFreq_Value,FDCANFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI48_VALUE,HSI_VALUE,HSPI1Freq_Value,HSPICLockSelection,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2C4Freq_Value,I2C5Freq_Value,I2C6Freq_Value,LPTIM2Freq_Value,LPUART1Freq_Value,LSCOPinFreq_Value,LSE_VALUE,LSIDIV_VALUE,LSI_VALUE,LTDCCLockSelection,LTDCFreq_Value,MCO1PinFreq_Value,MDF1Freq_Value,MSI_VALUE,OCTOSPIMFreq_Value,PLL2M,PLL2N,PLL2PoutputFreq_Value,PLL2QoutputFreq_Value,PLL2RoutputFreq_Value,PLL2Source,PLL3M,PLL3N,PLL3P,PLL3PoutputFreq_Value,PLL3QoutputFreq_Value,PLL3R,PLL3RoutputFreq_Value,PLL3Source,PLLDSIFreq_Value,PLLDSIIDF,PLLDSINDIV,PLLDSIODF,PLLDSIVCOFreq_Value,PLLM,PLLN,PLLPoutputFreq_Value,PLLQoutputFreq_Value,PLLRCLKFreq_Value,PLLSourceVirtual,RNGFreq_Value,SAESFreq_Value,SAI1Freq_Value,SAI2Freq_Value,SDMMCFreq_Value,SPI1Freq_Value,SPI2Freq_Value,SPI3Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USART6Freq_Value,USBPHYFreq_Value,VCOInput2Freq_Value,VCOInput3Freq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOPLL2OutputFreq_Value,VCOPLL3OutputFreq_Value
RCC.LPTIM2Freq_Value=160000000
RCC.LPUART1Freq_Value=160000000
RCC.LSCOPinFreq_Value=32000
RCC.LSE_VALUE=32768
RCC.LSIDIV_VALUE=32000
RCC.LSI_VALUE=32000
RCC.LTDCCLockSelection=RCC_LTDCCLKSOURCE_PLL3
RCC.LTDCFreq_Value=25000000
RCC.MCO1PinFreq_Value=160000000
RCC.MDF1Freq_Value=160000000
RCC.MSI_VALUE=4000000
RCC.OCTOSPIMFreq_Value=160000000
RCC.PLL2M=4
RCC.PLL2N=66
RCC.PLL2PoutputFreq_Value=132000000
RCC.PLL2QoutputFreq_Value=132000000
RCC.PLL2RoutputFreq_Value=132000000
RCC.PLL2Source=RCC_PLLSOURCE_HSE
RCC.PLL3M=4
RCC.PLL3N=125
RCC.PLL3P=8
RCC.PLL3PoutputFreq_Value=62500000
RCC.PLL3QoutputFreq_Value=250000000
RCC.PLL3R=20
RCC.PLL3RoutputFreq_Value=25000000
RCC.PLL3Source=RCC_PLLSOURCE_HSE
RCC.PLLDSIFreq_Value=500000000
RCC.PLLDSIIDF=DSI_PLL_IN_DIV4
RCC.PLLDSINDIV=125
RCC.PLLDSIODF=DSI_PLL_OUT_DIV2
RCC.PLLDSIVCOFreq_Value=1000000000
RCC.PLLM=4
RCC.PLLN=80
RCC.PLLPoutputFreq_Value=160000000
RCC.PLLQoutputFreq_Value=160000000
RCC.PLLRCLKFreq_Value=160000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.RNGFreq_Value=48000000
RCC.SAESFreq_Value=48000000
RCC.SAI1Freq_Value=132000000
RCC.SAI2Freq_Value=132000000
RCC.SDMMCFreq_Value=160000000
RCC.SPI1Freq_Value=160000000
RCC.SPI2Freq_Value=160000000
RCC.SPI3Freq_Value=160000000
RCC.SYSCLKFreq_VALUE=160000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=160000000
RCC.UART5Freq_Value=160000000
RCC.USART1Freq_Value=160000000
RCC.USART2Freq_Value=160000000
RCC.USART3Freq_Value=160000000
RCC.USART6Freq_Value=160000000
RCC.USBPHYFreq_Value=160000000
RCC.VCOInput2Freq_Value=4000000
RCC.VCOInput3Freq_Value=4000000
RCC.VCOInputFreq_Value=4000000
RCC.VCOOutputFreq_Value=320000000
RCC.VCOPLL2OutputFreq_Value=264000000
RCC.VCOPLL3OutputFreq_Value=500000000
SH.GPXTI5.0=GPIO_EXTI5
SH.GPXTI5.ConfNb=1
STMicroelectronics.X-CUBE-FREERTOS.1.0.1.CMSISJjRTOS2_Checked=true
STMicroelectronics.X-CUBE-FREERTOS.1.0.1.IPParameters=configENABLE_FPU,configUSE_APPLICATION_TASK_TAG,configTOTAL_HEAP_SIZE,configUSE_IDLE_HOOK,RTOS2CcCMSISJjRTOS2JjCore,RTOS2CcCMSISJjRTOS2JjHeap
STMicroelectronics.X-CUBE-FREERTOS.1.0.1.RTOS2CcCMSISJjRTOS2JjCore=TZIiNonIiSupported
STMicroelectronics.X-CUBE-FREERTOS.1.0.1.RTOS2CcCMSISJjRTOS2JjHeap=HeapIi4
STMicroelectronics.X-CUBE-FREERTOS.1.0.1.configENABLE_FPU=1
STMicroelectronics.X-CUBE-FREERTOS.1.0.1.configTOTAL_HEAP_SIZE=80000
STMicroelectronics.X-CUBE-FREERTOS.1.0.1.configUSE_APPLICATION_TASK_TAG=1
STMicroelectronics.X-CUBE-FREERTOS.1.0.1.configUSE_IDLE_HOOK=1
STMicroelectronics.X-CUBE-FREERTOS.1.0.1_SwParameter=RTOS2CcCMSISJjRTOS2JjHeap\:HeapIi4;RTOS2CcCMSISJjRTOS2JjCore\:TZIiNonIiSupported;
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.ApplicationCcGraphicsJjApplication=TouchGFXOoGenerator
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.GraphicsJjApplication_Checked=true
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.IPParameters=tgfx_display_interface,tgfx_vsync,tgfx_hardware_accelerator,tgfx_nemap_accelerator,tgfx_buffering_strategy,tgfx_vector_rendering,tgfx_oswrapper,tgfx_video,tgfx_video_strategy,tgfx_video_width,tgfx_video_height,tgfx_vector_fonts,ApplicationCcGraphicsJjApplication
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_buffering_strategy=Double
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_display_interface=disp_ltdc
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_hardware_accelerator=dma_2d
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_nemap_accelerator=gpu2d_enabled
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_oswrapper=CMSIS V2
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_vector_fonts=Enabled
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_vector_rendering=Hardware
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_video=Hardware
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_video_height=480
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_video_strategy=0
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_video_width=800
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1.tgfx_vsync=vsync_ltdc
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1_IsPackSelfContextualization=true
STMicroelectronics.X-CUBE-TOUCHGFX.4.24.1_SwParameter=ApplicationCcGraphicsJjApplication\:TouchGFXOoGenerator;
VP_CRC_VS_CRC.Mode=CRC_Activate
VP_CRC_VS_CRC.Signal=CRC_VS_CRC
VP_DCACHE1_VS_DCACHE.Mode=DCACHE_Activate
VP_DCACHE1_VS_DCACHE.Signal=DCACHE1_VS_DCACHE
VP_DCACHE2_VS_DCACHE.Mode=DCACHE_Activate
VP_DCACHE2_VS_DCACHE.Signal=DCACHE2_VS_DCACHE
VP_DMA2D_VS_DMA2D.Mode=DMA2D_Activate
VP_DMA2D_VS_DMA2D.Signal=DMA2D_VS_DMA2D
VP_GPDMA1_VS_GPDMACH0.Mode=SIMPLEREQUEST_GPDMACH0
VP_GPDMA1_VS_GPDMACH0.Signal=GPDMA1_VS_GPDMACH0
VP_GPDMA1_VS_GPDMACH1.Mode=SIMPLEREQUEST_GPDMACH1
VP_GPDMA1_VS_GPDMACH1.Signal=GPDMA1_VS_GPDMACH1
VP_GPU2D_VS_GPU2D.Mode=GPU2D_Activate
VP_GPU2D_VS_GPU2D.Signal=GPU2D_VS_GPU2D
VP_ICACHE_VS_ICACHE.Mode=DirectMappedCache
VP_ICACHE_VS_ICACHE.Signal=ICACHE_VS_ICACHE
VP_JPEG_VS_JPEG.Mode=JPEG_Activate
VP_JPEG_VS_JPEG.Signal=JPEG_VS_JPEG
VP_LPBAMQUEUE_VS_QUEUE.Mode=QUEUEMODE
VP_LPBAMQUEUE_VS_QUEUE.Signal=LPBAMQUEUE_VS_QUEUE
VP_LPBAM_VS_SIG1.Mode=SmartRun
VP_LPBAM_VS_SIG1.Signal=LPBAM_VS_SIG1
VP_LPBAM_VS_SIG4.Mode=LPDMA1
VP_LPBAM_VS_SIG4.Signal=LPBAM_VS_SIG4
VP_MEMORYMAP_VS_MEMORYMAP.Mode=CurAppReg
VP_MEMORYMAP_VS_MEMORYMAP.Signal=MEMORYMAP_VS_MEMORYMAP
VP_PWR_VS_DBSignals.Mode=DisableDeadBatterySignals
VP_PWR_VS_DBSignals.Signal=PWR_VS_DBSignals
VP_PWR_VS_LPOM.Mode=PowerOptimisation
VP_PWR_VS_LPOM.Signal=PWR_VS_LPOM
VP_PWR_VS_SECSignals.Mode=Security/Privilege
VP_PWR_VS_SECSignals.Signal=PWR_VS_SECSignals
VP_STMicroelectronics.X-CUBE-FREERTOS_VS_CMSISJjRTOS2_10.4.6_1.0.1.Mode=CMSISJjRTOS2
VP_STMicroelectronics.X-CUBE-FREERTOS_VS_CMSISJjRTOS2_10.4.6_1.0.1.Signal=STMicroelectronics.X-CUBE-FREERTOS_VS_CMSISJjRTOS2_10.4.6_1.0.1
VP_STMicroelectronics.X-CUBE-TOUCHGFX_VS_GraphicsJjApplication_4.24.1.Mode=GraphicsJjApplication
VP_STMicroelectronics.X-CUBE-TOUCHGFX_VS_GraphicsJjApplication_4.24.1.Signal=STMicroelectronics.X-CUBE-TOUCHGFX_VS_GraphicsJjApplication_4.24.1
VP_SYS_VS_tim6.Mode=TIM6
VP_SYS_VS_tim6.Signal=SYS_VS_tim6
board=custom
rtos.0.ip=STMicroelectronics.X-CUBE-FREERTOS.1.0.1
rtos.0.tasks.0=allocationType,Dynamic;bufferName,NULL;codeGen,Default;controlBlockName,NULL;entry,StartDefaultTask;name,defaultTask;parameter,NULL;priority,osPriorityNormal;stackSize,128
rtos.0.tasks.1=allocationType,Dynamic;bufferName,NULL;codeGen,As external;controlBlockName,NULL;entry,TouchGFX_Task;name,GUI_Task;parameter,NULL;priority,osPriorityNormal;stackSize,8192
